		WINDOWS 95/98 DRIVER RELEASE NOTES 
		FOR COLORSHOT DIGITAL PHOTO PRINTER 


1) First, turn off your PC and install the ColorShot Digital 
   Photo Printer by connecting it to a parallel port on your 
   PC and then plugging in its power supply. Next, boot up 
   your PC and follow the instructions below.

   NOTE: The ColorShot printer must be connected to your PC and 
   turned ON before you attempt to install the Windows 95/98 
   driver.

2) Driver Installation Procedure:

	a) Click the "Start" button, select "Settings", 
	   and then click on "Printers".  The Printers
	   window will appear.
	b) Double-click on the "Add Printer" icon.  This
	   will start up the Add Printer Wizard.
	c) Follow the instructions displayed by the 
	   Wizard, and select "Local Printer".
	d) When the Wizard displays a list of printer
	   manufacturers and models, click on the 
	   "Have Disk..." button.
	e) A dialog box titled "Install From Disk"
	   will appear.  Click on the "Browse" button
	   and then double-click on the folder name into 
	   which you had downloaded and unzipped the 
	   "colorshot_win.zip" file.  This should cause
	   the file "ppegasus.inf" to appear in the 
	   "File name" box. If it does, click on "OK".
	f) Once you have returned to the "Install From
	   Disk" dialog box with the folder name appearing
	   in the "Copy manufacturer's files from:" box,
	   click on "OK".
	g) You will return to the "Add Printer Wizard"
	   window, with "Polaroid Photo Printer Parallel" 
	   selected in the "Printers:" box.  Click "Next>".
	h) The Wizard will begin copying driver files,
	   and then ask for a port to be used with
	   the ColorShot printer.  Select a line printer
	   port (e.g. LPT1:), and click on "Next>".
	i) Follow subsequent instructions, select
	   your preferences, and then click on "Finish".
	j) Next, a "Setup" box will appear.  Click on 
	   the "Browse" button, and select the "SETUP.EXE"
	   application which is located in the IQA folder
	   below the folder into which you had downloaded 
	   and unzipped the "colorshot_win.zip" file. Click 
	   "Open".
	k) Now the "Setup" box will display the path pointing
	   to the "SETUP.EXE" application in the IQA folder.
	   Click "OK" in the "Setup" box.
	l) Some additional files will be set up. Follow the 
	   instructions which appear, and then click on "Finish".
	m) This completes the installation of the ColorShot Digital
	   Photo Printer driver for Windows 95/98.  Shut
	   down and reboot your PC now.

3) If, at any time, your ColorShot printer fails to print, 
   reset it by disconnecting the power cord at the rear of 
   the printer and then reconnecting it after waiting for 
   approximately ten seconds.
